Installation Guide of CAMA C Library and Driv er pac k age (V ersion 2.0.29c) for Lin ux OS and ISA/PCI-CC7x00

L\ <! Bh 1 >O Ho w to install 3 1.1 P ac k age V ersion : : : : : : : : : : : : : : : : : : : : : : : : : : 3 1.2 Directories : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 3 1.3 Before making : : : : : : : : : : : : : : : : : : : : : : : : : : 4 1.4 Ho w to mak e : : : : : : : : : : : : : : : : : : : : : : : : : : : 5 Bh 2 >O Sample programs 7 2.1 Ho w to mak e sample programs : : : : : : : : : : : : : : : : : 7 2.2 List of sample programs : : : : : : : : : : : : : : : : : : : : : 8 2.2.1 cratetest : : : : : : : : : : : : : : : : : : : : : : : : : : 8 2.2.2 single16 : : : : : : : : : : : : : : : : : : : : : : : : : : 8 2.2.3 single24 : : : : : : : : : : : : : : : : : : : : : : : : : : 8 2.2.4 bloac k16 : : : : : : : : : : : : : : : : : : : : : : : : : : 8 2.2.5 bloac k24 : : : : : : : : : : : : : : : : : : : : : : : : : : 8 2.2.6 w aitlam : : : : : : : : : : : : : : : : : : : : : : : : : : 8 Bh 3 >O Library reference 9 3.1 COPEN : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 9 3.2 CCLOSE : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 9 3.3 CRESET : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 9 3.4 CSETBR : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 10 3.5 CSETCR : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 10 3.6 CGENZ : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 10 3.7 CGENC : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 10 3.8 CSETI : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 11 3.9 CREMI : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 11 3.10 CAMA C : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 11 3.11 CAMA CW : : : : : : : : : : : : : : : : : : : : : : : : : : : : 12 3.12 CDMAL : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 12 3.13 CDMA W : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 13 3.14 CENLAM : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 13 3.15 CDSLAM : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 14 1

3.16 CWTLAM : : : : : : : : : : : : : : : : : : : : : : : : : : : : 14 3.17 NAF : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 14 Bh 4 >O I/O prot map 15 4.1 ISAcc7000 Register map : : : : : : : : : : : : : : : : : : : : : 15 4.2 ISAcc7700 Register map : : : : : : : : : : : : : : : : : : : : : 18 4.3 PCIcc7700 Register map : : : : : : : : : : : : : : : : : : : : : 21 Bh 5 >O Memo and Bugs 25 5.1 Memo : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : : 25 5.1.1 Commands : : : : : : : : : : : : : : : : : : : : : : : : 25 5.1.2 Files : : : : : : : : : : : : : : : : : : : : : : : : : : : : 25 5.2 Kno wn Bugs : : : : : : : : : : : : : : : : : : : : : : : : : : : 26 5.2.1 Common : : : : : : : : : : : : : : : : : : : : : : : : : 26 5.2.2 ISAcc7000 : : : : : : : : : : : : : : : : : : : : : : : : : 26 5.2.3 ISAcc7000 : : : : : : : : : : : : : : : : : : : : : : : : : 26 5.2.4 PCIcc7700 : : : : : : : : : : : : : : : : : : : : : : : : : 26 2

Bh 1 >O Ho w to install 1.1 P ac k age V ersion K\ %Q %C %1 !< %8 $K $O El MN %F %/ %K %+ <R @= $N \ISAcc7000" , \ISAcc7700" ,\PCIcc7700" $r Lin ux OS >e $G ;HMQ $9 $k $? $a $N %I %i %$ %P5Z $S %i %$ %V %i %j $, 4^$^ $l$F$$$^ $9 !# 3’$5 $s$, F~ <j $7 $? %Q%C%1 !< %8 $N L> A0 $O \camac.lin ux.X.X.XX.Y.tgz" $N 7A $H $J $C $F $$ $k $H ;W$$ $^$9 ( $3$3$G X $O ?t ;z Y $O 1Q 8l$N >. J8 ;z#1 J8 ;z $r I= $9 ) !# \camac.lin ux" $N 8e $K B3 $/ 3 $D $N ?t CM $O 3+ H/ $, 9T$o $l $? Lin ux $N OS %P !< %8 %g %s $G !" :G8e $K $/$C$D $$ $F$$ $k1Q8l$NJ8;z $, $3 $N%Q%C%1!< %8 $N%P !< %8 %g %s $K $"$?$j$^$9 !# Nc $( $P \camac.lin ux.2.0.29a.tgz" $G $" $l $P !" Lin ux 2.0.29 $G 3+H/$5 $l $? \a" %P !< %8 %g %s $N%Q%C%1!< %8$r I= $7 $^$9 !# $b$A$m $s $N$3$H !" F1 $8 \a" %P !< %8 %g %s $N%Q %C%1!< %8$G $b \camac.lin ux" $N 8e $K B3$/ 3 $D$N ?tCM $, 0[ $J $l $P A4 $/0c $&FbMF $K$J $C $F$$ $^$9 !# %Q%C%1!< %8 $N ?tCM $H 3’$5 $s $, ;H$C $F$$ $k Lin ux $N%P!< %8 %g %s $N ?tCM $H$N4X78 $G $9 $, !" ;O $a$N 2 $D$N?tCM $, 0lCW $7 $F $$ $l $P $* $= $i $/F0 :n $9$k $H ;W $o $l $^$9 !# ( $G$- $l $P 3 $D$N?tCM $, 0lCW $7 $F$$ $k $3$H $, K>$^ $7 $$ !# ) 1.2 Directories $^ $: F~<j $7 $?%Q %C%1!< %8$r E83+ $7 $^$9 !# $3$N %I %- %e %a %s %H $r FI $s$G $$ $k J} $O $b $& %Q%C%1!< %8 $r E83+ $7 $F $$ $k $H $O ;W$$$^$9 $, !" % tar -tvzf camac.linux.X.X.XX.Y.tgz � � � � � $G E83+$9$k;v $,$G $- $^$9 !# $9$k $H E83+ $r 9T$C $? %G %# %l %/ %H %j0J2< $K !" ------ camaclinux.X.X.XX.Y --- src | +--- include | +--- lib | +--- doc | +--- samples --- src | +--- bin 3

List 1.2.1: \Directories tree" $3$NMM $J %G %# %l %/ %H %j $, :n @. $5 $l $k $O $: $G$9!# (\camac.X.X.XX.Y" $N %G %# %l %/ %H %j $r 0J2< %H %C %W %G %# %l %/ %H %j $H 8F $S $^$9 !# ) 1.3 Before making <B:] $K %i %$ %V %i %j !< $H %I %i %$ %P !< $r :n@.$9$k<j=g $O !" 1. %H %C %W %G %# %l %/ %H %j $K$" $k Mak e�le $N JT=8 2. %H %C %W %G %# %l %/ %H %j $G mak e clean $N <B9T 3. %H %C %W %G %# %l %/ %H %j $G mak e dep $N <B9T 4. %H %C %W %G %# %l %/ %H %j $G mak e Src $N <B9T 5. %H %C %W %G %# %l %/ %H %j $G mak e install $N <B9T $H$J $C $F$$ $^$9 !# Mak e�le $N 0lItJ, $r 0J2< $K <( $7 $F $*$-$^$9 !# # File Name : Makefile # Introduction : Makefile for Crate Controller "ISA/PCI-cc7x00" on Linux OS. # : Main version. # Creation Date : 1997/08/19 # Author : Yasu.S Yamagata Univ. department of physics. # Modified by : # Version : 2.0.29a # # User Selection. # # Crate Controller(Select from ISAcc7000 , ISAcc7700 or PCIcc7700) CRATETYPE = PCIcc7700 # CC7x00_MAJOR = "30" # Base Address of Crate Controller ADDRESS = "0x0310" # Irq of Crate Controller. IRQ = "10" # Debug Option DEBUG = # # Do not edit following lines. # SHELL = /bin/sh CC7x00_TOP = $(shell pwd) INCDIR = $(CC7x00_TOP)/include 4

LIBDIR = $(CC7x00_TOP)/lib List 1.3.2: \Mak e�le" JT =8 $9 $Y $- It J, $O !" \CRA TETYPE" , \CC7x00 MAJOR" , \ADDRESS" , \IR Q" \DEBUG" $N ItJ, $G $9!# ( ?tCM $r ;X Dj$9 $k It J, $K $D $$$F$O \ " $G 0O $‘ $N$r K: $l $J $$ $G 2<$5$$ !# ) 1. CRA TENAME: $3$N9T $O !" ;H MQ $9 $k %/ %l !< %H %3 %s %H %m!< %i!< $NA* Br It J, $G $9!# I, $: \ISAcc7000" \ISAcc7700" \PCIcc7700" $N 3 $D$N Cf $+$i 1 $D$r A* $s $G 2<$5$$ !# 2. CC7x00 MAJOR: $3$N9T $G $O :n@. $9$k %I %i %$ %P $N %a %8 %c !< %J %s%P $r;XDj $7 $^$9!# \/usr/src/lin ux/include/lin ux/ma jor.h" $r8+ $F ;H $o $l $F $$ $J $$ $b $N $rA* Br $7 $F 3d$jEv $F$F 2<$5$$ !# 3. ADDRESS: $3$N9T $G $O %/ %l !< %H %3 %s %H %m!< %i !< $N I/O P ort $N %Y!<%9 %" %I %l %9 $r ;XDj $7 $^$9!# % more /proc/ioports � � � � � $r <B 9T $7 !" 6u $$ $F $$ $k %]!< %H$rA* Br $7 $F3d $j Ev $F $F2< $5 $$!# \PCIcc7700" $r A*Br $7 $? >l9g $G$b$3$N CM $O I,MW $G $9$N $G !" I, $: ;XDj $7 $F 2<$5$$ !# 4. IR Q: $3 $N 9T $G $O ;HMQ$9$k IR Q $r ;XDj $7 $^$9!# % more /proc/ioports � � � � � $r<B 9T $7 !" 6u $$ $F $$ $k IR Q $r;X Dj $7$F 2< $5 $$ !# \PCIcc7700" $rA* Br $7$? >l 9g $G $b $3 $N CM $OI, MW $G $9 $N $G !" I, $:;X Dj $7$F 2< $5 $$ !# $? $@ $7 !" \PCIcc7700" $r A*Br $7 $? >l9g !" IR Q $K \10" $r @_Dj$9$k $H%7 %9 %F%‘ $, %O %s %0 %" %C %W $9 $k $3$H $, 3NG’$5 $l $F $$$^$9!# 5. DEBUG: $3$N 9T $G$O 2?$b;XDj $7 $J $$ $G 2<$5$$ !# J#?t $N%/ %l !< %H %3 %s %H %m!< %i!< MQ $N %I %i %$ %P 5Z $S %i %$ %V %i %j $r :n @. $9$k ?M $O !" %i %$ %V %i %j!<$H %I %i %$ %P !<$r :n @. $9 $k <j =g$N (1) $+ $i (5) $r 7+ $j JV $7 $F 2< $5$$ !# 1.4 Ho w to mak e Mak e�le $NJT =8 $, =* $C $? $i<B :] $K %I %i %$ %P $H %i %$ %V %i %j $r:n @. $7 $^ $9 !# %H%C %W %G %# %l %/ %H %j $K 0\F0 $7 !" 5

% make clean � � � � � % make dep � � � � � % make Src � � � � � $H <B9T $7 $^$9 !# $3 $l $G %i %$ %V %i %j5Z $S %I %i %$ %P $, %H %C %W %G %# %l %/ %H %j $N 2< $K $" $k \lib" %G %# %l %/ %H %j $K :n@.$5 $l $?$O $:$G $9!# $G$O !" <B:] $K :n @. $7 $? %I %i %$ %P 5Z $S %i %$ %V %i %j $N %$ %s %9 %H !< %k$G$9 $, !" ro ot 8"8B $r ;} $D %f!<%6 $G 9T $J$$ $^$9 !# % su � � � � � Ey $r MQ$$ $F ro ot 8"8B $r ;}$D %f!<%6 $K$J $C $? 8e !" % make install � � � � � $r <B9T$9 $k $H !" \/dev" %G %# %l %/ %H %j $N Cf $K %I %i %$ %P $, !" \/usr/lib" $N Cf $K %i %$ %V %i %jEy $, %$ %s %9 %H !< %k $5 $l $^$9 !# 6

Bh 2 >O Sample programs 2.1 Ho w to mak e sample programs K\ %Q %C %1!< %8$K $O !" %9%$ %C %A %l%8 %9 %? $H %$ %s %?!< %i %W%H %l%8 %9 %? $rMQ $$ $? !" %i %$ %V %i %j !<5Z $S %I %i %$ %P !<$N%F %9 %H MQ%5 %s %W %k %W %m %0 %i %‘ $, ImB0 $7 $F $$$^ $9!# %I %i %$ %P !< 5Z $S %i %$ %V %i %j !< $, %$ %s %9 %H !< %k $5 $l $? 8e !" $3 $l$i $N%5 %s %W %k %W %m %0 %i %‘ $r :n@.$9$k $3$H $, 2DG= $K$J $j $^$9 !# :n@. $9$k<j=g $O !" 1. \camac.lin ux.X.X.XX.Y/samples/src" $K $" $k testlib drv.h $N JT=8 2. %H %C %W %G %# %l %/ %H %j $G mak e Samples $N <B9T $H$J $C $F$$ $^$9 !# 0J 2< $K<( $9 \testlib drv.h" $NIt J, $G !" ;H MQ $9 $k %9%$ %C %A %l%8 %9 %? $H %$ %s%? !< %i %W%H%l %8 %9 %? $N %9 %F!< %7 %g %s %J %s %P$r Dj5A $7 $F 2<$5$$ !# /* For single16/24 and block 16/24 */ /* station number of switch register */ #define SW_REG 4 /* For waitlam */ /* station number of interrupt register */ #define INTERRUPT_REG 2 List 2.1.1: \testlib drv.h" \testlib drv.h" $N JT=88e !" %H %C %W %G %# %l %/ %H %j $G % make Samples � � � � � $H <B9T $9$k $H !" \camac.lin ux.X.X.XX.Y/samples/bin" $K %5 %s %W %k %W %m %0 %i %‘ $, :n@.$5 $l $^$9 !# 7

2.2 List of sample programs 2.2.1 cratetest %/ %l !< %H %3 %s %H %m!< %i !< $^ $o$j $N %U %! %s %/ %7%g %s ( %*!< %W%s !" %/ %m!< %: !" %j %; %C %H Ey ) $N%F %9 %H %W %m %0 %i %‘ $G $9!# 2.2.2 single16 %9 %$ %C %A %l %8 %9 %? $K BP $7 16 bit %G !<%?$N =q$- 9~ $_ / FI$_9~$_ $r 7+$j JV $7 $^ $9!# =q $-9~$^ $l $k %G !<%? $O 0 $+$i ;O$^ $C $F 0x� $^ $G %$ %s %/%j %a %s %H $5 $l $F 9T$-$^$9 !# 2.2.3 single24 %9 %$ %C %A %l %8 %9 %? $K BP $7 24 bit %G !<%?$N =q$- 9~ $_ / FI$_9~$_ $r 7+$j JV $7 $^ $9!# =q $- 9~$^ $l $k %G !<%? $O 0 $+$i ;O$^$C $F 0x� $^ $G %$ %s %/%j %a %s %H $5 $l $F 9T$-$^$9 !# 2.2.4 bloac k16 16 bit %V %m %C %/ %" %/ %7 %g %s $N%F %9 %H $G $9 !# %9 %$ %C %A %l %8 %9 %? $r MQ$$$^$9 !# 2.2.5 bloac k24 24 bit %V %m %C %/ %" %/ %7 %g %s $N%F %9 %H $G $9 !# %9 %$ %C %A %l %8 %9 %? $r MQ$$$^$9 !# 2.2.6 w aitlam 3d$j9~ $_4X78 $N %F %9 %H $G $9!# %$ %s %?!<%i %W%H%l %8 %9 %? $N%5 %V %" %I %l %9 0 HV $K E,Ev $J%Q %k %9 $r %/ %m%C %/ %8 %’%M %l !<%? Ey $+$i F~ $l $F 2<$5$$ !# 8

Bh 3 >O Library reference 3.1 COPEN NAME COPEN De�ned Name CAM Op en CAMOPN Abstract Op en the CAMA C crate con troller. Syn tax in t COPEN(v oid) Argumen ts Nothing. Return V alue Successful : 0 (CC K READ Y) F alse : 1 (CC K BUSY) de�ned b y \camlib.h" 3.2 CCLOSE NAME CCLOSE De�ned Name CAM Close CAMCLS Abstract Close the CAMA C crate con troller. Syn tax in t COPEN(v oid) Argumen ts Nothing. Return V alue Successful : 0 F alse : It returns gro v al v alue \errno" de�ned b y \errno.h" 3.3 CRESET NAME CRESET De�ned Name Abstract Reset the CAMA C crate con troller. Syn tax in t CRESET(v oid) Argumen ts Nothing. Return V alue 0 In the case of using \ISAcc7000", this function is n ull function, so this function alw a ys returns 0. 9

3.4 CSETBR NAME CSETBR De�ned Name Abstract Setting curren t branc h n um b er. Syn tax in t CSETBR(in t No) Argumen ts No : Branc h’s No. Return V alue This function is not supp orted. So alw a ys this function returns 0. 3.5 CSETCR NAME CSETCR De�ned Name Abstract Setting curren t crate n um b er. Syn tax in t CSETCR(in t No) Argumen ts No : crate’s No. Return V alue Successful : 0 F alse : EINV AL de�ned b y \errno.h" 3.6 CGENZ NAME CGENZ De�ned Name Abstract Initializing the curren t CAMA C crate. Syn tax in t CGENZ(v oid) Argumen ts Nothing. Return V alue 0 3.7 CGENC NAME CGENC De�ned Name Abstract Clearing the data w a y of curren t CAMA C crate. Syn tax in t CGENC(v oid) Argumen ts Nothing. Return V alue 0 10

3.8 CSETI NAME CSETI De�ned Name Abstract Setting the data w a y inhibit of curren t CAMA C crate. Syn tax in t CSETI(v oid) Argumen ts Nothing. Return V alue 0 3.9 CREMI NAME CREMI De�ned Name Abstract Resetting the data w a y inhibit of curren t CAMA C crate. Syn tax in t CSETI(v oid) Argumen ts Nothing. Return V alue 0 3.10 CAMA C NAME CAMA C De�ned Name CAMA CL Abstract Executing single CAMA C op eration with 24-bit CAMA C data. Syn tax in t CAMA C(in t naf, v oid* data, in t* q, in t* x) Argumen ts naf : NAF data created b y NAF() function. data : P oin ter of in teger data. q : P oin ter of in teger data. (If it is set 0, there is no Q resp onse.) x : P oin ter of in teger data. (If it is set 0, there is no X resp onse.) Return V alue 0 11

3.11 CAMA CW NAME CAMA CW De�ned Name Abstract Executing single CAMA C op eration with 16-bit CAMA C data. Syn tax in t CAMA CW(in t naf, v oid* data, in t* q, in t* x) Argumen ts naf : NAF data created b y NAF() function. data : P oin ter of short in teger data. q : P oin ter of in teger data. (If it is set 0, there is no Q resp onse.) x : P oin ter of in teger data. (If it is set 0, there is no X resp onse.) Return V alue 0 3.12 CDMAL NAME CDMAL De�ned Name CamBloLonW AIt CBL W AI Abstract Executing blo c k CAMA C op eration with 24-bit CAMA C data. Syn tax in t CDMAL(in t mo de, in t naf, v oid* bu�er, in t length, in t* ret len,in t err) Argumen ts mo de : Mo de of blo c k action. CC K MODES QSTOP : Q stop mo de. CC K MODES IGNR Q : ignore Q mo de. CC K MODES REPEA T : Q rep eat mo de. CC K MODES ASCAN : Address scan mo de. bu�er : p oin ter of in teger data arra y . length : Maxm um length of data bu�er b y coun ting a in teger. ret len : Length of writting or reading data b y coun ting in teger. err : P oin ter os in teger data. (Q and X resp onse.) If it is set 0 : Q and X If it is set 1 : no Q and X If it is set 2 : Q and no X If it is set 3 : no Q and no X Return V alue 0 12

3.13 CDMA W NAME CDMA W De�ned Name CamBloW orW AIt CBWW AI Abstract Executing blo c k CAMA C op eration with 16-bit CAMA C data. Syn tax in t CDMA W(in t mo de, in t naf, v oid* bu�er, in t length, in t* ret len,in t err) Argumen ts mo de : Mo de of blo c k action. CC K MODES QSTOP : Q stop mo de. CC K MODES IGNR Q : ignore Q mo de. CC K MODES REPEA T : Q rep eat mo de. CC K MODES ASCAN : Address scan mo de. naf : NAF data created b y NAF() function. bu�er : P oin ter of short in teger data arra y . length : Maxm um length of data bu�er b y coun ting a short in teger. ret len : Length of writting or reading data b y coun ting short in teger. err : P oin ter os in teger data. Q and X resp onse. If it is set 0 : Q and X If it is set 1 : no Q and X If it is set 2 : Q and no X If it is set 3 : no Q and no X Return V alue 0 3.14 CENLAM NAME CENLAM De�ned Name CAM EnableLAM CELAM Abstract Enabling in terrupt of curren t crate con troller. Syn tax in t CENLAM(in t LamP attern) Argumen ts LamP attern : In teger data. (This is 24-bit data) If bit is 1, enabling LAM. If bit is 0, disbling LAM. ex) A t LamP attern is 0x00000013. Enabling in terrupt b y mo dules station No 1, 2, and 5. Return V alue 0 13

3.15 CDSLAM NAME CENLAM De�ned Name CAM DisbleLAM CDLAM Abstract Disabling in terrupt of curren t crate con troller. Syn tax in t CDSLAM(v oid) Argumen ts Nothing. Return V alue 0 3.16 CWTLAM NAME CWTLAM De�ned Name CAM W aitLAM CWLAM Abstract W aitnig for generating LAM on curren t crate. Syn tax in t CWTLAM(in t time) Argumen ts time : In teger data. W aitnig time.(m sec) Return V alue 0 : Successful ETIMEOUT : Time out o ccured. EINV AL : Unexp ected LAM o ccured. de�ned b y \errno.h" In the case of using \PCIcc7700", this function is not supp oted no w. 3.17 NAF NAME De�ned Name NAF Abstract Generating CAMA C address data b y using \n", \a" and \f ". Syn tax in t NAF(in t n, in t a, in t f ) Argumen ts n : Station n um b er. a : Sub address. f : CAMA C function. Return V alue Compressed address data for this library functions. 14

Bh 4 >O I/O prot map 4.1 ISAcc7000 Register map O�set -00h- DLR BIT W rite Read 15 W16 : Data Bit 16 R16 : Data Bit 16 14 W15 : Data Bit 15 R15 : Data Bit 15 13 W14 : Data Bit 14 R14 : Data Bit 14 12 W13 : Data Bit 13 R13 : Data Bit 13 11 W12 : Data Bit 12 R12 : Data Bit 12 10 W11 : Data Bit 11 R11 : Data Bit 11 09 W10 : Data Bit 10 R10 : Data Bit 10 08 W09 : Data Bit 09 R09 : Data Bit 09 07 W08 : Data Bit 08 R08 : Data Bit 08 06 W07 : Data Bit 07 R07 : Data Bit 07 05 W06 : Data Bit 06 R06 : Data Bit 06 04 W05 : Data Bit 05 R05 : Data Bit 05 03 W04 : Data Bit 04 R04 : Data Bit 04 02 W03 : Data Bit 03 R03 : Data Bit 03 01 W02 : Data Bit 02 R02 : Data Bit 02 00 W01 : Data Bit 01 R01 : Data Bit 01 O�set -01h- CCR 07 | | 06 | | 05 | | 04 | | 03 | | 02 | | 01 CA2 : Crate Address \2" | 00 CA1 : Crate Address \1" | 15

O�set -02h- DHR BIT W rite Read 15 | | 14 | | 13 | | 12 | | 11 | | 10 | | 09 | | 08 | | 07 W24 : Data Bit 24 R24 : Data Bit 24 06 W23 : Data Bit 23 R23 : Data Bit 23 05 W22 : Data Bit 22 R22 : Data Bit 22 04 W21 : Data Bit 21 R21 : Data Bit 21 03 W20 : Data Bit 20 R20 : Data Bit 20 02 W19 : Data Bit 19 R19 : Data Bit 19 01 W18 : Data Bit 18 R18 : Data Bit 18 01 W17 : Data Bit 17 R17 : Data Bit 17 O�set -04h- NAFLR/LAMLR Bit W rite Read 15 | L16 : LAM Station 16 14 | L15 : LAM Station 15 13 | L14 : LAM Station 14 12 | L13 : LAM Station 13 11 A8 : SubAddress \8" L12 : LAM Station 12 10 A4 : SubAddress \4" L11 : LAM Station 11 09 A2 : SubAddress \2" L10 : LAM Station 10 08 A1 : SubAddress \1" L09 : LAM Station 09 07 | L08 : LAM Station 08 06 | L07 : LAM Station 07 05 | L06 : LAM Station 06 04 N16 : Station Num b er \16" L05 : LAM Station 05 03 N08 : Station Num b er \08" L04 : LAM Station 04 02 N04 : Station Num b er \04" L03 : LAM Station 03 01 N02 : Station Num b er \02" L02 : LAM Station 02 00 N01 : Station Num b er \01" L01 : LAM Station 01 16

O�set -06h- CSR/LAMHR/NAFHR BIT W rite Read 15 LI : LAM In ternal LI : LAM In ternal 14 | LS : LAM Sum 13 | ONL : On Line 12 | DNE : Done 11 EI : Enable In terrupt EI : Enable In terrupt 10 I : Inhibit I : Inhibit 09 Z : Initialize NX : NO-X 08 C : Clear NQ : NO-Q 07 | L24 : LAM Station 24 06 | L23 : LAM Station 23 05 | L22 : LAM Station 22 04 F16 : F unction co de \16" L21 : LAM Station 21 03 F08 : F unction co de \08" L20 : LAM Station 20 02 F04 : F unction co de \04" L19 : LAM Station 19 01 F02 : F unction co de \02" L18 : LAM Station 18 00 F01 : F unction co de \01" L17 : LAM Station 17 O�set -07h- EXER 07 | | 06 | | 05 | | 04 | | 03 | | 02 | | 01 | | 00 | | !{ ISAcc7000 %/ %l !< %H %3 %s %H %m !<%i!< <h07@bL@=q $h$j H4?h 17

4.2 ISAcc7700 Register map O�set -00h- CSR Bit W rite Read 15 | | 14 | | 13 | | 12 | | 11 | | 10 | | 09 | | 08 | | 07 LI : LAM In ternal LI : LAM In ternal 06 RS : Reset LS : LAM Sum 05 | ONL : On Line 04 | DNE : Done 03 EI : Enable In terrupt EI : Enable In terrupt 02 I : InhiBit I : InhiBit 01 Z : Initialize NX : NO-X 00 C : Clear NQ : NO-Q O�set -02h- CCR/LAMLR Bit W rite Read 15 | L16 : LAM Station 16 14 | L15 : LAM Station 15 13 | L14 : LAM Station 14 12 | L13 : LAM Station 13 11 | L12 : LAM Station 12 10 | L11 : LAM Station 11 09 | L10 : LAM Station 10 08 | L09 : LAM Station 09 07 | L08 : LAM Station 08 06 | L07 : LAM Station 07 05 | L06 : LAM Station 06 04 | L05 : LAM Station 05 03 | L04 : LAM Station 04 02 CA04 : Crate Address \04" L03 : LAM Station 03 01 CA02 : Crate Address \02" L02 : LAM Station 02 00 CA01 : Crate Address \01" L01 : LAM Station 01 18

O�set -04h- NAFR/LAMHR Bit W rite Read 15 | | 14 | | 13 N16 : Station Num b er \16" | 12 N08 : Station Num b er \08" | 11 N04 : Station Num b er \04" | 10 N02 : Station Num b er \02" | 09 N01 : Station Num b er \01" | 08 A08 : SubAddress \08" | 07 A04 : SubAddress \04" L24 : LAM Station 24 06 A02 : SubAddress \02" L23 : LAM Station 23 05 A01 : SubAddress \01" L22 : LAM Station 22 04 F16 : F unction co de \16" L21 : LAM Station 21 03 F08 : F unction co de \08" L20 : LAM Station 20 02 F04 : F unction co de \04" L19 : LAM Station 19 01 F02 : F unction co de \02" L18 : LAM Station 18 00 F01 : F unction co de \01" L17 : LAM Station 17 O�set -06h- DLR Bit W rite Read 15 W16 : Data Bit 16 R16 : Data Bit 16 14 W15 : Data Bit 15 R15 : Data Bit 15 13 W14 : Data Bit 14 R14 : Data Bit 14 12 W13 : Data Bit 13 R13 : Data Bit 13 11 W12 : Data Bit 12 R12 : Data Bit 12 10 W11 : Data Bit 11 R11 : Data Bit 11 09 W10 : Data Bit 10 R10 : Data Bit 10 08 W09 : Data Bit 09 R09 : Data Bit 09 07 W08 : Data Bit 08 R08 : Data Bit 08 06 W07 : Data Bit 07 R07 : Data Bit 07 05 W06 : Data Bit 06 R06 : Data Bit 06 04 W05 : Data Bit 05 R05 : Data Bit 05 03 W04 : Data Bit 04 R04 : Data Bit 04 02 W03 : Data Bit 03 R03 : Data Bit 03 01 W02 : Data Bit 02 R02 : Data Bit 02 00 W01 : Data Bit 01 R01 : Data Bit 01 19

O�set -08h- DHR Bit W rite Read 15 | | 14 | | 13 | | 12 | | 11 | | 10 | | 09 | | 08 | | 07 W24 : Data Bit 24 R24 : Data Bit 24 06 W23 : Data Bit 23 R23 : Data Bit 23 05 W22 : Data Bit 22 R22 : Data Bit 22 04 W21 : Data Bit 21 R21 : Data Bit 21 03 W20 : Data Bit 20 R20 : Data Bit 20 02 W19 : Data Bit 19 R19 : Data Bit 19 01 W18 : Data Bit 18 R18 : Data Bit 18 00 W17 : Data Bit 17 R17 : Data Bit 17 O�set -0Ah- EXER Bit W rite Read 15 | | 14 | | 13 | | 12 | | 11 | | 10 | | 09 | | 08 | | 07 | | 06 | | 05 | | 04 | | 03 | | 02 | | 01 | | 00 | | !{ ISAcc7700 %/ %l !< %H %3 %s %H %m !<%i!< <h07@bL@=q $h$j H4?h 20

4.3 PCIcc7700 Register map O�set -00h- CSR BIT W rite Read 31 | | 30 | | 29 | | 28 | | 27 | | 26 | | 25 | | 24 | | 23 | | 22 | | 21 | | 20 | | 19 | | 18 | | 17 | | 16 | | 15 | | 14 | | 13 | | 12 | | 11 | | 10 | | 09 | | 08 | | 07 LI : LAM In ternal LI LAM In ternal 06 RS : Reset LS : LAM Sum 05 | ONL : On Line 04 | DNE : Done 03 EI : Enable In terrupt EI : Enable In terrupt 02 I : Inhibit I : Inhibit 01 Z : Initialize NX : NO-X 00 X : Clear NQ : NO-Q 21

O�set -04h- CCR/LAMR/NAFR BIT W rite Read 31 | | 30 | | 29 | | 28 | | 27 | | 26 | | 25 | | 24 | | 23 | LAM Station 24 22 | LAM Station 23 21 | LAM Station 22 20 | LAM Station 21 19 | LAM Station 20 18 CA4 : Crate Address \04" LAM Station 19 17 CA2 : Crate Address \02" LAM Station 18 16 CA1 : Crate Address \01" LAM Station 17 15 | LAM Station 16 14 | LAM Station 15 13 N16 : Station Num b er \16" LAM Station 14 12 N08 : Station Num b er \08" LAM Station 13 11 N04 : Station Num b er \04" LAM Station 12 10 N02 : Station Num b er \02" LAM Station 11 09 N01 : Station Num b er \01" LAM Station 10 08 A08 : Sub Address \08" LAM Station 09 07 A04 : Sub Address \04" LAM Station 08 06 A02 : Sub Address \02" LAM Station 07 05 A01 : Sub Address \01" LAM Station 06 04 F16 : F unction co de \16" LAM Station 05 03 F08 : F unction co de \08" LAM Station 04 02 F04 : F unction co de \04" LAM Station 03 01 F02 : F unction co de \02" LAM Station 02 00 F01 : F unction co de \01" LAM Station 01 22

O�set -08h- DR BIT W rite Read 31 | | 30 | | 29 | | 28 | | 27 | | 26 | | 25 | | 24 | | 23 W24 : Data Bit 24 R24 : Data Bit 24 22 W23 : Data Bit 23 R23 : Data Bit 23 21 W22 : Data Bit 22 R22 : Data Bit 22 20 W21 : Data Bit 21 R21 : Data Bit 21 19 W20 : Data Bit 20 R20 : Data Bit 20 18 W19 : Data Bit 19 R19 : Data Bit 19 17 W18 : Data Bit 18 R18 : Data Bit 18 16 W17 : Data Bit 17 R17 : Data Bit 17 15 W16 : Data Bit 16 R16 : Data Bit 16 14 W15 : Data Bit 15 R15 : Data Bit 15 13 W14 : Data Bit 14 R14 : Data Bit 14 12 W13 : Data Bit 13 R13 : Data Bit 13 11 W12 : Data Bit 12 R12 : Data Bit 12 10 W11 : Data Bit 11 R11 : Data Bit 11 09 W10 : Data Bit 10 R10 : Data Bit 10 08 W09 : Data Bit 09 R09 : Data Bit 09 07 W08 : Data Bit 08 R08 : Data Bit 08 06 W07 : Data Bit 07 R07 : Data Bit 07 05 W06 : Data Bit 06 R06 : Data Bit 06 04 W05 : Data Bit 05 R05 : Data Bit 05 03 W04 : Data Bit 04 R04 : Data Bit 04 02 W03 : Data Bit 03 R03 : Data Bit 03 01 W02 : Data Bit 02 R02 : Data Bit 02 00 W01 : Data Bit 01 R01 : Data Bit 01 23

O�set -0Ch- EXER BIT W rite Read 31 | | 30 | | 29 | | 28 | | 27 | | 26 | | 25 | | 24 | | 23 | | 22 | | 21 | | 20 | | 19 | | 18 | | 17 | | 16 | | 15 | | 14 | | 13 | | 12 | | 11 | | 10 | | 09 | | 08 | | 07 | | 06 | | 05 | | 04 | | 03 | | 02 | | 01 | | 00 | | !{ PCIcc7700 %/ %l !< %H %3 %s %H %m !<%i!< <h07@bL@=q $h$j H4?h 24

Bh 5 >O Memo and Bugs 5.1 Memo 5.1.1 Commands 1. /bin/mkno d : %9 %Z %7%c%k%U%! %$ %k$r :n@.$9$k !# 2. /sbin/insmo d : %m!< %@%V %k %b %8 %e !< %k$N %m!< %I !# ex) ****.o $, $" $k %G %# %l %/ %H %j $G !" % insmod **** � � � � � $H <B9T$9$k $H%b %8 %e !< %k \****.o" $N%m !< %I $r 9T $J $& !# 3. /sbin/rmmo d : %m!< %@%V %k %b %8 %e !< %k$N%" %s %m!< %I !# ex) insmo d $G %m!< %I $7 $? %b %8 %e !< %k \****.o" $N%" %s %m !< %I !# % rmmod **** � � � � � 4. mak e Src : %I %i %$ %P$H%i %$ %V %i %j $N:n@. !# 5. mak e Samples : %5 %s %W %k $N :n@. !# 6. mak e dep : mak e MQ4D6- %U %! %$ %k $N :n@. !# 7. mak e clean : %G %# %l %/ %H %j $N@6A] 8. mak e force clean : %G %# %l %/ %H %j $N 6/@)@6A] 9. mak e install : %i %$ %V %i %j !" %I %i %$ %P$N %$ %s %9 %H !< %k 10. mak e uninstall : %i %$ %V %i %j !" %I %i %$ %P$N%" %s %$ %s %9 %H !< %k 11. mak e force uninstall : %i %$ %V %i %j !" %I %i %$ %P$N 6/@) %" %s %$ %s %9 %H !< %k 12. mak e load : %I %i %$ %P$N%m !< %I 13. mak e unload : %I %i %$ %P$N%" %s %m !< %I 5.1.2 Files 1. /pro c/devices : 8=:_%m!< %I $5 $l $F $$ $k %G %P %$ %9 $N 0lMw !# 2. /pro c/in terrupts : IR Q $N 0lMw !# 3. /pro c/iop orts : I/O P ort $N 0lMw !# 4. /pro c/p ci : PCI %G %P %$ %9 $N 0lMw !# 25

5. /pro c/v ersion : Lin ux $N%P!< %8 %g %s !# 6. /v ar/log/syslog : Lin ux $N k ernel $, EG$- =P$9 %a %C %;!< %8 !# ro ot 8"8B $, L5$$ $H 8+$k $3$H $, =PMh $J $$ !# 5.2 Kno wn Bugs 5.2.1 Common 1. $H$K$+ $/$^ $@$" $A $3 $A $K $$ $C $Q $$%P %0$, M-$k $O$:!# 5.2.2 ISAcc7000 1. LAM $, N)$C $F $$ $k 4V !" %I %i %$ %P !<$N 3d$j 9~$_ %k !<%A %s$, 2? 2s$b 8F $P $l B3 $1 $k !# 2r7h:v $H $7 $F !" 3d $j9~$_ %k !<%A %s $, 8F $P $l $? ;~E@ $G %/ %l !< %H %3 %s%H %m!<%i!< $r 3d$j9~ $_ IT2D>uBV $K JQ99 $7 $F $$ $k !# 5.2.3 ISAcc7000 1. :# $O $^ $@ 8+$D $+ $C $F$$$J$$ $, $I $3$+$K$" $k $O$:!# 5.2.4 PCIcc7700 1. %I %i %$ %P !< $r %m !< %I $9 $k $H $- $K IR Q 10 $rA* Br $7 $F %3 %s%Q %$ %k $5 $l$F $$ $k $H !" %7 %9 %F%‘ $, %O %s %0 %"%C %W $9$k !# 3+ H/ 4D 6- FC M- $NLdBj $+ $I $& $+ $O ITL@!# 2. %I %i %$ %P !<$N3d$j9~$_4X?t $, $^ $@ 40@. $7 $F $$$J$$ !# 26